

**Installing INFORMS LK-P12 Firmware**

Prerequisites:

* Install LK-P12 driver
1. Connect printer to PC
2. Launch the **FW DOWNLOAD PROGRAM**
3. Change Model to: **LK-P12**
4. Select Port: **USB** {Optionally COM port}
5. Select **FILE OPEN** & select the **LK-P12\_V1.14\_ZPL\_INFORMS.bin** or newer firmware file. Click **Open**.
6. Click **Printer F/W**.



1. You will see the following warning. Click **Yes**.



1. There will be a Downloading message on the printer and it will play a song at the conclusion. The printer will power down.
2. Click **OK** in the Download window.
3. Click **Exit**.
4. Power up printer. Press the Feed button. If the label does not feed to tear off then use the Mobile Label Printer Utility to set the printer to Gap.